../Core/Src/serial.c:58:22:uart3_log_hal_error	3
../Core/Src/serial.c:78:22:uart3_arm_rx_or_log	3
../Core/Src/serial.c:93:15:CCS_RxEventCallback	4
../Core/Src/serial.c:116:15:HAL_UART_ErrorCallback	5
../Core/Src/serial.c:134:6:CCS_SerialLoop	43
../Core/Src/serial.c:297:6:CCS_Init	1
../Core/Src/serial.c:311:26:crc16_ibm	3
../Core/Src/serial.c:326:17:CCS_BuildPacket	4
../Core/Src/serial.c:342:13:CCS_SendPacket	2
../Core/Src/serial.c:350:13:CCS_SendResetReason	1
../Core/Src/serial.c:354:6:CCS_SendEmergencyStop	1
../Core/Src/serial.c:358:6:CCS_SendStart	1
../Core/Src/serial.c:362:13:CCS_CalculateEnergy	2
../Core/Src/serial.c:377:13:send_state	3
../Core/Src/serial.c:405:26:expected_payload_len	2
../Core/Src/serial.c:421:22:apply_command	13
../Core/Src/serial.c:493:25:process_received_packet	8
../Core/Src/serial.c:546:13:CCS_UART3_Watchdog	3
