../Core/Src/serial.c:65:22:uart3_log_hal_error	3
../Core/Src/serial.c:85:22:uart3_arm_rx_or_log	3
../Core/Src/serial.c:100:15:CCS_RxEventCallback	4
../Core/Src/serial.c:123:15:HAL_UART_ErrorCallback	5
../Core/Src/serial.c:141:6:CCS_SerialLoop	62
../Core/Src/serial.c:342:6:CCS_Init	1
../Core/Src/serial.c:356:26:crc16_ibm	3
../Core/Src/serial.c:371:17:CCS_BuildPacket	4
../Core/Src/serial.c:387:13:CCS_SendPacket	2
../Core/Src/serial.c:395:13:CCS_SendResetReason	1
../Core/Src/serial.c:399:6:CCS_SendEmergencyStop	1
../Core/Src/serial.c:403:6:CCS_SendStart	1
../Core/Src/serial.c:407:13:CCS_CalculateEnergy	2
../Core/Src/serial.c:422:13:send_state	3
../Core/Src/serial.c:452:26:expected_payload_len	2
../Core/Src/serial.c:468:22:apply_command	15
../Core/Src/serial.c:550:25:process_received_packet	8
../Core/Src/serial.c:603:13:CCS_UART3_Watchdog	3
