../Drivers/CMSIS/Include/core_cm3.h:1762:34:__NVIC_SystemReset	1
../Core/Src/serial.c:52:6:CCS_RxEventCallback	4
../Core/Src/serial.c:62:6:CCS_SerialLoop	41
../Core/Src/serial.c:207:6:CCS_Init	1
../Core/Src/serial.c:219:17:crc16_ibm	4
../Core/Src/serial.c:234:17:CCS_BuildPacket	4
../Core/Src/serial.c:250:13:CCS_SendPacket	2
../Core/Src/serial.c:258:13:CCS_SendResetReason	1
../Core/Src/serial.c:262:6:CCS_SendEmergencyStop	1
../Core/Src/serial.c:266:6:CCS_SendStart	1
../Core/Src/serial.c:270:13:CCS_CalculateEnergy	2
../Core/Src/serial.c:285:13:send_state	2
../Core/Src/serial.c:312:17:expected_payload_len	11
../Core/Src/serial.c:328:13:apply_command	13
../Core/Src/serial.c:395:16:process_received_packet	6
