../Core/Src/serial.c:70:22:uart3_log_hal_error	3
../Core/Src/serial.c:90:22:uart3_arm_rx_or_log	3
../Core/Src/serial.c:106:15:CCS_RxEventCallback	4
../Core/Src/serial.c:129:15:HAL_UART_ErrorCallback	5
../Core/Src/serial.c:149:6:CCS_TxCpltCallback	4
../Core/Src/serial.c:165:6:CCS_SerialLoop	62
../Core/Src/serial.c:365:6:CCS_Init	1
../Core/Src/serial.c:380:26:crc16_ibm	3
../Core/Src/serial.c:395:17:CCS_BuildPacket	4
../Core/Src/serial.c:411:13:CCS_SendPacket	4
../Core/Src/serial.c:428:13:CCS_SendResetReason	1
../Core/Src/serial.c:432:6:CCS_SendEmergencyStop	1
../Core/Src/serial.c:436:6:CCS_SendStart	1
../Core/Src/serial.c:440:13:CCS_CalculateEnergy	2
../Core/Src/serial.c:455:13:send_state	3
../Core/Src/serial.c:485:26:expected_payload_len	2
../Core/Src/serial.c:501:22:apply_command	15
../Core/Src/serial.c:583:25:process_received_packet	8
../Core/Src/serial.c:636:13:CCS_UART3_Watchdog	4
../Core/Src/serial.c:649:13:CCS_LogUart3Error	1
